rotor_lift_coeff = 150;
engine_power = 1000;
max_engine_rpm = 1500;
max_thrust = 100;
max_rotor_rpm = 600;
max_rotor_pitch = 910;
min_rotor_pitch = -364;
ac_weight = 800;
start_fuel = 200;
pitch_control = 17;
roll_control = 30;
yaw_control = 8;
pitch_stability = 10;
roll_stability = 40;
yaw_stability = 100;
pitch_inertia = 250;
roll_inertia = 150;
yaw_inertia = 250;
pitch_drag = 40;
roll_drag = 40;
yaw_drag = 40;
x_drag = 200;
y_drag = 200;
clean_drag = 100;
gear_drag = 40;
test1 = 0;
test2 = 0;
test3 = 0;
